## Design Specifications

####

2-11

Item | Measurement | Qualification | Specification
DIMENSIONS | Overall length |  | 4,410 mm (163.0 in.)
Overall width |  | 1,695 mm (66.7 in.)
Overall height | without roof antenna | 1,425 mm (56.1 in.)
with roof antenna | 1,550 mm (61.0 in.)
Wheelbase (MPW condition) |  | 2,570 mm (101.2 in.)
Track (MPW condition) | Front | 1,469 mm (57.8 in.)
Rear | 1,472 mm (58.0 in.)
Ground clearance |  | 129.7 mm (5.11 in.)
Seating capacity |  | Four (4)
WEIGHT | Curb weight |  | 1,199-1,208 kg (2,643-2,663 lbs)
Max. permissible weight |  | 1,550 kg (3,417 lbs)
ENGINE | Type |  | Water-cooled, 4-stroke DOHC VTEC engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke |  | 86 x 86 mm (3.39 x 3.39 in.)
Displacement |  | 1,998 cm³ (122 cu in.)
Compression ratio |  | 11.0
Valve train |  | Chain drive, DOHC VTEC 4 valves per cylinder
Lubrication system |  | Forced wet sump, with trochoid pump
Oil pump displacement | at 6,000 engine rpm (min-1) | 54.3 litre (57.4 US qt, 47.8 Imp qt) per minute
Water pump displacement | at 6,000 engine rpm (min-1) | 82 litre (87 US qt, 72 Imp qt) per minute
Fuel required |  | Premium UNLEADED gasoline with 95 research octane number or higher

a a a