## Interior Trim

#### Headliner Removal/Installation

20-72

6. Install the carpet in the reverse order of removal, and note these items:

- Take care not to damage, wrinkle or twist the carpet.
- Make sure the seat harnesses are routed correctly.
- Slip the slit in the carpet over the hook.
- Replace the clip if it's damaged.
- Reattach the cut areas under the heater around the shift lever and parking brake lever with a wire tie.
- When installing new carpet, cut the carpet (A) under the heater area (B), and around the shift lever (C) and parking brake lever (D). After installing the new carpet, reattach the cut areas (C, D) with wire ties.