## Opening Repair Chart

####

4-12

Door and Windshield Openings:

Unit: mm (in.)

1. A

   Windshield lower dashboard guide pin

2. B, C

   Windshield opening flange notch (2 places)

3. D, E, F, G, H, I, J, K,

   Door opening flange notch (16 places)

Rear Window and Trunk Lip Openings:

1. L, M

   Rear window opening flange notch (3 places)

2. N

   Trunk gutter area convex bead

3. O

   Outer panel range end (2 places)

4. P

   Trunk seal flange water drain notch