## Seats

#### Front Seat Disassembly/Reassembly - With Manual Height Adjustable

20-89

For some models: SRS components are located in this area. Review the SRS component locations (see page 23-23), and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service.

NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- The left side seat is shown, the right side seat is symmetrical.

Disassemble the seat as shown.

Reassemble the seat in the reverse order of disassembly, and note these items:

- Apply multipurpose grease to the moving portion of the seat track.
- To prevent wrinkles in the seat cushion cover, stretch the material evenly over the pad.

  1. HOOKS

     (Five places)

  2. HOOKS
  3. Release the seat cushion cover from the cushion frame spring.
  4. HOOKS
  5. HEADREST
  6. SEAT-BACK
  7. SIDE AIRBAG HARNESS

     (For some models)

  8. WIRE TIE
  9. HOOK
  10. RECLINE COVER
  11. CLIP
  12. RECLINE KNOB
  13. HEIGHT HANDLE
  14. CAP
  15. CLIP
  16. HOOK
  17. CLIP
  18. SEAT HEATER UNIT

      (For some models)

  19. SLIDE LEVER
  20. SEAT CUSHION FRAME/SEAT TRACKS
  21. CLIP
  22. CENTRE COVER
  23. SEAT HEATER HARNESS

      (For some models)

  24. CLIP
  25. HANGER SPRING

      (With side airbag)