## Engine Block

#### Flywheel Removal and Installation

7-5

Special Tools Required Ring gear holder 07LAB-PV00100

1. Remove the transmission (see page 13-5).

1. Remove the eight flywheel bolts, then separate the flywheel from the crankshaft flange. After installation, tighten the bolts in a criss-cross pattern.

1. Inspect ring gear teeth for wear or damage

1. Install the transmission (see page 13-10).

a a a