## Intake Manifold and Exhaust System

#### Intake Manifold Removal and Installation (cont'd)

9-6

1. Install the air cleaner housing (A) and connect the IAT sensor connector (B).

1. Install the breather hose (C).

1. Install the EVAP canister hose (A), brake booster vacuum hose (B), and vacuum hoses (C).

1. Install the intake manifold cover.

1. Clean up any spilled engine coolant.

1. After installation, check that all tubes, hoses, and connectors are installed correctly.

1. Inspect for fuel leaks. Turn the ignition switch ON (II) (do not operate the starter) so that the fuel pump runs for about 2 seconds and pressurises the fuel line. Repeat this operation two or three times, then check for fuel leakage at any point in the fuel line.

1. Refill the radiator with engine coolant, and bleed air from the cooling system with the heater valve open (see page 10-6).

a a a