## Intake Air System

#### Throttle Body Removal/Installation

11-451

NOTE:

- Do not adjust the throttle stop screw.
- After reassembly, adjust the throttle cable (see page 11-449).
- The Throttle Position (TP) sensor is not removable.

  1. THROTTLE BODY
  2. THROTTLE STOP SCREW

     (Do not adjust)

  3. THROTTLE LEVER
  4. There should be no clearance
  5. THROTTLE CABLE
  6. EVAPORATIVE EMISSION (EVAP) CANISTER PURGE VALVE
  7. GASKET

     Replace.

  8. THROTTLE POSITION (TP) SENSOR
  9. IDLE AIR CONTROL (IAC) VALVE