## Shafts and Clutches

#### Clutch Disassembly

14-205

Special Tools Required

- Clutch spring compressor set, 07LAE-PX40000
  - Clutch spring compressor attachment, 07LAE-PX40100
  - Clutch spring compressor attachment, 07HAE-PL50101
  - Clutch spring compressor bolt assembly, 07GAE-PG40200

- Snap ring pliers, 07LGC-0010100

1. Remove the snap ring (A), then remove the clutch end plate, the clutch discs and the plates with a screwdriver (B).

2. Remove the wave spring from the 1st, 3rd and 4th clutches.

3. Remove the disc spring from the 1st-hold clutch (7-position).

4. Install the special tool on the clutch assembly.