## Driveline/Axle

#### Driveshafts Reassembly

16-9

Exploded View

1. Pack cavity with specified amount of grease.
2. SET RING, Replace.
3. INBOARD JOINT
4. CIRCLIP
5. ROLLER
6. SPIDER
7. INBOARD BOOT

   Pack cavity with specified amount of grease.

8. DOUBLE LOOP BAND, Replace.
9. Pack cavity with specified amount of grease.
10. DRIVESHAFT
11. STOP RING, Replace.
12. EAR CLAMP BANDS, Replace.
13. OUTBOARD JOINT
14. Pack cavity with specified amount of grease.
15. OUTBOARD BOOT (TPE)
16. DOUBLE LOOP BAND, Replace.
17. DYNAMIC DAMPER
18. Right driveshaft

a a a