## Idle Control System

#### Brake Pedal Position Switch Signal Circuit Troubleshooting (cont'd)

11-124

4. Inspect the No. 7 HORN, STOP (15A) fuse in the under-hood fuse/relay box.

Is the fuse OK?

YES | - Repair open in the wire between the brake pedal position switch and the No. 7 HORN, STOP (15 A) fuse. Inspect the brake pedal position switch (see page 19-10).
NO | - Repair short in the wire between the ECM/PCM (E22) and the No. 7 HORN, STOP (15A) fuse. Replace the No. 7 HORN, STOP (15A) fuse.