## Power Mirrors

#### Power Mirror Actuator Test

22-148

1. Remove the door panel (see page 20-142).

2. Disconnect the 8P[6P]connector (A) from the power mirror actuator (B).

4-door:

5-door:

3. Check actuator operation by connecting power and ground according to the table.

4. If the mirror fails to work properly, replace the mirror actuator.

Defogger Test:

5. Check for continuity between the No. 3 [No. 2] and No. 4 [No. 1] terminals of the 8P[6P]connector. There should be continuity.

[ ]: 5-door

Retract Switch:

6. Check actuator operation by connecting battery power and ground according to the table.

[ ] : Right Power Motor

7. If the retract actuator fails to work properly, replace the mirror.