## Intake Manifold and Exhaust System

#### Exhaust Pipe and Muffler Replacement

9-9

NOTE: Use new gaskets and self-locking nuts when reassembling.

1. GASKET

   Replace.

2. SELF-LOCKING NUT

   10 x 1.25 mm

   54 Nm (5.5 kgf/m, 40 lbf/ft)

   Replace.

3. MUFFLER
4. HEAT SHIELD
5. 6 x 1.0 mm

   9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)

6. EXHAUST PIPE B
7. GASKET

   Replace.

8. THREE WAY CATALYTIC CONVERTER (TWC)
9. GASKET

   Replace.

10. SELF-LOCKING NUT

    10 x 1.25 mm

    33 Nm (3.4 kgf/m, 25 lbf/ft)

    Replace.

11. SELF-LOCKING NUT

    8 x 1.25 mm

    18 Nm (1.8 kgf/m, 13 lbf/ft)

    Replace.

12. SELF-LOCKING NUT

    10 x 1.25 mm

    33 Nm (3.4 kgf/m, 25 lbf/ft)

    Replace.

13. SELF-LOCKING NUT

    10 x 1.25 mm

    54 Nm (5.5 kgf/m, 40 lbf/ft)

    Replace.

14. EXHAUST PIPE A
15. GASKET

    Replace.

16. 8 x 1.25 mm

    22 Nm (2.2 kgf/m, 16 lbf/ft)

17. SELF-LOCKING NUT

    10 x 1.25 mm

    33 Nm (3.4 kgf/m, 25 lbf/ft)

    Replace.

a a a