## Standards and Service Limits

#### Steering

2-9

Item | Measurement | Qualification | Standard or New | Service Limit
Steering wheel | Rotational play measured at outside edge | With engine running | 0-10 mm (0-0.39 in.) | -
Starting load measured at outside edge | With engine running | 29 N (3.0 kgf, 6.6 lbs) | -
Gearbox | Angle of rack guide screw loosened from locked position |  | 15° Max. |

Suspension

Item | Measurement | Qualification | Standard or New | Service Limit
Wheel alignment | Camber | Front | 0°00' + 45'
Rear | -0°45' + 45'
Caster | Front | 1°33' + 1°
Total Toe | Front | 0 +3 mm (0 +0.12 in.)
Rear | Adjust: IN 2+2 -1 mm (0.08+0.08 -0.04 in.) Inspect: IN 2 + 3 mm (0.08 + 0.12 in.)
Front wheel turning angle | Inside wheel | 40°00' + 2°
Outside wheel | 31°00' (Reference)
Aluminium wheel | Runout | Axial | 0-0.7 mm (0-0.03 in.) | 2.0 mm (0.08 in.)
Radial | 0-0.7 mm (0-0.03 in.) | 1.5 mm (0.06 in.)
Steel wheel | Runout | Axial | 0-1.0 mm (0-0.04 in.) | 2.0 mm (0.08 in.)
Radial | 0-1.0 mm (0-0.04 in.) | 1.5 mm (0.06 in.)
Wheel bearing | End play | Front | 0-0.05 mm (0-0.002 in.)
Rear | 0-0.05 mm (0-0.002 in.)

a a a