## Rear Side Outer Panel

#### Installation

3-8

1. Glue the insulator to the centre inner pillar as shown.

Insulator: P/N. 774416-SF1-000

Adhesive: Cemedine 366, or equivalent.

1. CENTRE INNER PILLAR
2. INSULATOR

1. Set the new centre pillar stiffener lower into position and install the middle floor gusset.

1. NEW CENTRE PILLAR STIFFENER LOWER
2. MIDDLE FLOOR GUSSET

3. Set the new repair part (outer panel) and rear pillar gutter lower into position and clamp them.

Check the body dimensions (see section 4).

- Remove the repair part (outer panel) and weld the centre pillar stiffener lower.

1. NEW CENTRE PILLAR STIFFENER LOWER
2. CENTRE PILLAR STIFFENER UPPER

4. Tack weld the outer panel and rear pillar gutter lower.
5. Temporarily install the door, tailgate and rear bumper and check for differences in level and clearance.

Make sure the body lines flow smoothly.

a a a