## Seat

#### Rear Seat-back Cover Replacement (cont'd)

20-241

Rear Seat Cushion Cover Replacement

11. Pull back the edge of the seat-back cover (A) all the way around and release the clips (B), then remove the seat-back cover. The right seat-back is shown, the left seat-back is similar.

12. Install the cover in the reverse order of removal and note these items:

- To prevent wrinkles when installing a seat-back cover, make sure the material is stretched evenly over the pad before securing the hooks and clips.
- On right seat-back with centre shoulder belt: When installing the seat-back frame to the pad, slip the centre belt through the hole in the seat-back cover and pad.
- Replace any clips you removed with new ones. Install them with commercially available upholstery ring pliers.

NOTE: The right seat cushion is shown, the left seat cushion is similar.

1. Remove the rear seat cushion (see page 20-237).
2. Release all the retainer strips (A) from under the seat cushion and fold back the seat cushion cover (B), then remove the cushion mat (C).