## Cylinder Head

#### Cylinder Head Removal (cont'd)

6-12

7. Remove the brake booster vacuum hose (A) and positive crankcase ventilation (PCV) hose (B).

8. Relieve fuel pressure, refer to the '01 Civic Shop Manual on this CD (see page 11-130).
9. Remove the EVAP canister hose.

10. Remove the ground cable (A), upper radiator hose (B), lower radiator hose (C), heater hose (D) and water bypass hose (E).

11. Remove the two bolts securing the connecting pipe, then remove the connecting pipe from the water passage.