## Interior Lights

#### Spotlights Test/ Replacement - Without Sunroof

22-138
Ceiling Light Test/Replacement

1. Turn the light switch OFF.

2. Carefully pry off the lenses (A) with a small screwdriver.

   Spotlight: | 8 W x 2

3. Remove the two mounting screws.
4. Disconnect the 2P connector (B) from the housing (C).
5. Check for continuity between the terminals in each switch position according to the table.

6. When installing the spotlights housing, if the threads in the ET screw are worn out, use an oversized ET screw made specifically for this application.

1. Turn the light switch OFF.

2. Carefully pry off the lens (A) with a small screwdriver.

   Ceiling Light: | 8 W

3. Remove the two mounting screws.
4. Disconnect the 3P connector (B) from the housing (C).
5. Check for continuity between the terminals in each switch position according to the table.

6. When installing the ceiling light housing, if the threads in the ET screw are worn out, use an oversized ET screw made specifically for this application.