## Fuel and Emissions Systems

#### System Descriptions (cont'd)

11-20

Vacuum Hose Routing

No. | Part Name | QTY | Remarks
(1) | JOINT; 4WAY | 1 |
(2) | HOSE; VACUUM, V/PIPE-4WAY | 1 | ø7
(3) | HOSE; VACUUM, TURBO-EVRV | 1 | ø10
(4) | HOSE; VACUUM, 4WAY-EVRV (TURBO) | 1 | ø7-ø8 4WAY-EVRV (TURBO)
(5) | HOSE; VACUUM, 4WAY-EVRV (EGR) | 1 | ø7-ø8 4WAY-EVRV (EGR)
(6) | HOSE; VACUUM, 4WAY-VSV | 1 | ø7-ø8 4WAY-VSV
(7) | HOSE; VACUUM, VSS-VSV | 1 | ø7-ø8 VSS-VSV
(8) | HOSE; VACUUM, EGR V-EVRV | 1 | ø10
(9) | JOINT; 3WAY | 1 |
(10) | HOSE; VACUUM, EGR-3WAY | 1 | ø10
(11) | HOSE; VACUUM, 3WAY-A/C | 1 | ø10
(12) | CLIP; HOSE, VACUUM | 1 | ø7-ø7
(13) | CLIP; HOSE, VACUUM | 2 | ø7-ø10
(14) | CLIP; HOSE, VACUUM | 1 | ø10-ø10

a a a