## Standards and Service Limits

#### Automatic Transmission and A/T Differential (cont'd)

2-20

Item | Measurement | Qualification | Standard or New | Service Limit
Countershaft | Diameter of needle bearing contact area | at left end | 36.004-36.017 mm (1.4175-1.4180 in.) | When worn or damaged
at 3rd gear | 35.980-35.996 mm (1.4165-1.4172 in.) | When worn or damaged
at 4th gear | 27.980-27.993 mm (1.1016-1.1021 in.) | When worn or damaged
at reverse gear collar | 31.975-31.991 mm (1.2589-1.2595 in.) | When worn or damaged
at 1st gear collar | 31.975-31.991 mm (1.2589-1.2595 in.) | When worn or damaged
I.D. of gears | 1st gear | 38.000-38.016 mm (1.4961-1.4967 in.) | When worn or damaged
3rd gear | 41.000-41.016 mm (1.6142-1.6148 in.) | When worn or damaged
4th gear | 33.000-33.016 mm (1.2992-1.2998 in.) | When worn or damaged
Reverse gear | 38.000-38.016 mm (1.4961-1.4967 in.) | When worn or damaged
End play of gears | 1st gear | 0.1-0.5 mm (0.004-0.020 in.) | -
3rd gear | 0.05-0.17 mm (0.002-0.007 in.) | -
4th gear | 0.10-0.18 mm (0.004-0.007 in.) | -
Reverse gear | 0.10-0.25 mm (0.004-0.010 in.) | -
28 mm distance collar length | No. 1 | 39.00 mm (1.535 in.) | -
No. 2 | 39.10 mm (1.539 in.) | -
No. 3 | 39.20 mm (1.543 in.) | -
No. 4 | 39.30 mm (1.547 in.) | -
No. 5 | 39.05 mm (1.537 in.) | -
No. 6 | 39.15 mm (1.541 in.) | -
No. 7 | 39.25 mm (1.545 in.) | -
No. 8 | 38.90 mm (1.531 in.) | -
No. 9 | 38.95 mm (1.533 in.) | -
3rd gear collar length |  | 20.65-20.70 mm (0.8130-0.8150 in.) | -
Reverse gear collar length |  | 14.5-14.6 mm (0.571-0.575 in.) | -
Reverse gear collar flange thickness |  | 2.4-2.6 mm (0.094-0.102 in.) | When worn or damaged
1st gear collar length |  | 14.5-14.6 mm (0.571-0.575 in.) | -
1st gear collar flange thickness |  | 2.4-2.6 mm (0.094-0.102 in.) | When worn or damaged
3rd gear splined washer thickness |  | 4.95-5.00 mm (0.195-0.197 in.) | When worn or damaged
3rd clutch feed pipe O.D. | At 15 mm (0.6 in.) from end | 7.97-7.98 mm (0.3138-0.3142 in.) | 7.95 mm (0.313 in.)
3rd clutch feed pipe bushing I.D. |  | 8.000-8.022 mm (0.3150-0.3158 in.) | 8.03 mm (0.316 in.)
Reverse selector hub O.D. |  | 51.87-51.90 mm (2.042-2.043 in.) | When worn or damaged
1st gear I.D. of one-way clutch contact area |  | 83.339-83.365 mm (3.2810-3.2821 in.) | When worn or damaged
Park gear diameter of one-way clutch area |  | 66.685-66.698 mm (2.6254-2.6259 in.) | When worn or damaged

a a a