## Engine Block

#### Crankshaft Installation (cont'd)

7-24
Oil Pan Installation

19. Clean and dry the oil pump mating surfaces.
20. Install the oil pump (A).

1. Install a new crankshaft oil seal in the oil pump (see step 12 on page 8-11).
2. Apply liquid gasket, part No. 08C70-K0234M, 08C70-K0334M or 08C70-X0331S, evenly to the block mating surface of the oil pump and to the inner threads of the bolt holes.
3. Grease the lip of the oil seal and apply oil to the new O-ring (B).
4. Install the dowel pins (C), then align the inner rotor with the crankshaft and install the oil pump.
5. Clean the excess grease off the crankshaft and check the seal for distortion.

21. Install the oil screen (D) with a new gasket (E).
22. Install the oil pan (see page 7-24).

Aluminium Oil Pan Type:

1. Clean and dry the oil pan mating surfaces and bolt holes.
2. Apply liquid gasket, part No. 08C70-K0334M or 08C70-X0331S, evenly to the oil pan mating surface of the block and to the inner threads of the bolt holes.

NOTE:

- Apply liquid gasket 4 mm wide.
- Apply liquid gasket doubly to the jointing point of the liquid gasket.

1. Apply liquid gasket along the broken line.

3. Install the oil pan.
4. Tighten the bolts in 2 or 3 steps. In the final step, tighten all bolts, in sequence to 12 Nm (1.2 kgf/m, 8.7 lbf/ft).

5. After assembly, wait at least 30 minutes before filling the engine with oil.