## Design Specifications

####

2-18

Item | Measurement | Qualification | Specification
DIMENSIONS | Overall length |  | 4,285 mm (168.7 in.)
Overall width |  | 1,695 mm (66.7 in.)
Overall height | without roof antenna | 1,495 mm (58.9 in.)
with roof antenna | 1,585 mm (62.2 in.)
Wheelbase | KE, KG, KR, KS models (MPW condition) | 2,685 mm (105.7 in.)
KY model | 2,680 mm (105.5 in.)
Track | Front KE, KG, KR, KS models (MPW condition) | 1,472 mm (58.0 in.)
Front KY model | 1,470 mm (57.9 in.)
Rear KE, KG, KR, KS models (MPW condition) | 1,489 mm (58.6 in.)
Rear KY model | 1,470 mm (57.9 in.)
Ground clearance |  | 104 mm (4.10 in.)
Seating capacity |  | Five (5)
WEIGHT | Curb Weight | (M/T) | 1,130-1,195 kg (2,491-2,634 lbs)
(A/T) | 1,164-1,1221 kg (2,566-2,692 lbs)
Max. permissible Weight | European models | 1,620-1,660 kg (3,570-3,660 lbs)
ENGINE | Type | D14Z6 engine | Water-cooled, 4-stroke SOHC engine
D16V1, D16V3 engines | Water-cooled, 4-stroke SOHC VTEC engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke | D14Z6 engine | 75 x 79 mm (2.95 x 3.11 in.)
D16V1, D16V3 engines | 75 x 90 mm (2.95 x 3.54 in.)
Displacement | D14Z6 engine | 1,396 cm3 (85 cu in.)
D16V1, D16V3 engines | 1,590 cm3 (97 cu in.)
Compression ratio | D14Z6 engine | 10.4
D16V1 engine | 9.4
D16V3 engine | 10.4
Valve train | D14Z6 engine | Belt driven, SOHC 4 valves per cylinder
D16V1, D16V3 engines | Belt driven, SOHC VTEC 4 valves per cylinder
Lubrication system |  | Forced, wet sump, with trochoid pump
Oil pump displacement | at 6,000 engine rpm (min-1) | 36.4 l (38.5 US qt, 32.0 imp qt) per minute
Water pump displacement | at 6,000 engine rpm (min-1) | 130 l (137 US qt, 114 imp qt)/minute
Fuel required | KE, KG, KR, KS models | UNLEADED gasoline with 95 research octane number or higher
KY model | LEADED gasoline with 91 research octane number or higher (RON of 91 UNLEADED gasoline may also be used)