## PGM-FI System

#### MIL Circuit Troubleshooting (cont'd)

11-268

27. Check for continuity between the fuel pump 5P connector terminal No. 5 and body ground.

FUEL PUMP 5P CONNECTOR

Wire side of female terminals

Is there continuity?

YES | - Repair short in the wire between the fuel pump and the PGM-FI main relay 2. Also replace the No. 17 FUEL PUMP (15A) fuse.
NO | - Go to step 28.

28. Reinstall the PGM-FI main relay 2 (A).

LHD model:

RHD model:

29. Check for continuity between the fuel pump 5P connector terminal No. 5 and body ground.

FUEL PUMP 5P CONNECTOR

Wire side of female terminals

Is there continuity?

YES | - Replace the PGM-FI main relay 2. Also replace the No. 17 FUEL PUMP (15A) fuse.
NO | - Check the fuel pump, and replace it as necessary. Also replace the No. 17 FUEL PUMP (15A) fuse.

30. Disconnect ECM/PCM connector E (31P).
31. Turn the ignition switch ON (II).
32. Measure voltage between ECM/PCM connector terminals E9 and body ground.

ECM/PCM CONNECTOR E (31P)

Wire side of female terminals

Is there battery voltage?

YES | - Go to step 33.
NO | - Repair open in the wire between the No. 17 FUEL PUMP (15A) fuse and the ECM/PCM (E9).