## SRS

#### SRS Indicator Light Circuit Troubleshooting (cont'd)

23-156

7. Disconnect the U3o connector (A) from the SRS unit.

8. Connect a voltmeter between the No. 14 terminal (+) of C1 connector and body ground. Turn the ignition switch ON (II), and measure voltage. There should be 0.5 V or less.

C1 CONNECTOR

Wire side of female terminals

Is voltage as specified?

YES - Faulty SRS unit; replace the SRS unit.

NO - Short to power in the PNK wire of dashboard wire harness A or in the floor wire harness; replace the faulty harness.

9. Turn the ignition switch OFF. Check the No. 19 (7.5A) fuse in the under-dash fuse/relay box.

Did fuse No. 19 (7.5A) blow?

YES - Go to step 12.

NO - Go to step 10.

10. Disconnect the C2 connector (A) from the gauge assembly.