## SRS

#### SRS Indicator Light Circuit Troubleshooting (cont'd)

23-148

The SRS Indicator Light Stays On After the Ignition Switch is Turned ON (II) (4-door Model)

1. Erase the DTC memory (see page 23-38).

Does the SRS indicator light go off while the DTC memory is erased?

YES - Go to step 42.

NO - Go to step 2.

2. Check the No. 13 (10A) fuse in the under-dash fuse/relay box.

Is the fuse OK?

YES - Go to step 19.

NO - Go to step 3.

3. Replace the No. 13 (10A) fuse in the under-dash fuse/relay box.
4. Turn the ignition switch ON (II) and wait for 30 seconds. Then turn the ignition switch OFF.
5. Check the No. 13 (10A) fuse in the under-dash fuse/relay box.

Is the fuse OK?

YES - The system is OK at this time.

NO - Go to step 6.

6. Replace the No. 13 (10A) fuse in the under-dash fuse/relay box.
7. Disconnect the battery negative cable and wait for 3 minutes.

8. Disconnect the D1o connector.

9. Disconnect the P1o connector.