## Seats

#### Rear Seat-back Latch Replacement – Folding Type

20-97

Rear Seat-back Lock Cylinder/Knob Replacement - Folding Type

NOTE: Take care not to scratch the interior trim.

1. Remove the rear shelf (see page 20-65).
2. Disconnect the cylinder rod (A), and remove the bolts, then remove the seat-back latch (B).

   Fastener Locations
   : Bolt, 2

3. Install the latch in the reverse order of removal, and note these items:

- Make sure the cylinder rod is connected securely.
- Make sure the seat-back locks securely and opens properly.

NOTE:

- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to scratch the interior trim.
- The lock cylinder is shown, the knob is similar.

1. Remove the lock cylinder trim (A).

2. From trunk compartment, disconnect the cylinder rods from both seat-back latches.
3. Remove the screws, then remove the seat-back lock cylinder/knob (A) and cylinder rods (B).

   Fastener Locations
   : Screw, 2

4. Install the lock cylinder/knob in the reverse order of removal, and note these items:

- Make sure the cylinder rod is connected securely.
- Make sure the seat-back opens properly.