## Intake Manifold and Exhaust System

#### Exhaust Pipe and Muffler Replacement

9-8

NOTE: Use new gaskets and self-locking nuts when reassembling.

1. GASKET, Replace
2. MUFFLER
3. 8 x 1.25 mm, 22 Nm (2.2kgf/m, 16 lbf/ft), Replace

   Tighten the bolts in steps alternating side-to-side

4. EXHAUST PIPE B
5. HEAT SHIELD
6. GASKET, Replace
7. SECONDARY HEATED OXYGEN SENSOR (SECONDARY HO2S)

   44 Nm (4.5 kgf/m, 33 lbf/ft)

8. THREE WAY CATALYTIC CONVERTER (TWC)
9. PRIMARY HEATED OXYGEN SENSOR (PRIMARY HO2S)

   44 Nm (4.5 kgf/m, 33 lbf/ft)

10. 8 x 1.25 mm, 22 Nm (2.2 kgf/m, 16 lbf/ft), Replace

    Tighten the bolts insteps alternating side-to-side

11. GASKET, Replace
12. SELF-LOCKING NUT, 10 x 1.25 mm, 33 Nm (3.4 kgf/m, 25 lbf/ft), Replace

a a a