## Power Steering

#### Fluid Leakage Inspection

17-22

NOTE: LHD type is shown, RHD type is symmetrical.

1. GEARBOX and VALVE BODY UNIT

   Check for leaks at the mating surface and flare nut connections.

2. HOSES and LINES

   Inspect hoses for damage, leaks, interference and twisting.

   Inspect fluid lines for damage, rusting and leakage.

   Check for leaks at hose and line joints and connections.

3. PUMP ASSEMBLY

   Check for leaks at the pump seal, inlet and outlet fittings.