## Keyless/Power Door Lock System

#### Door Lock Actuator Test

22-236

Driver's door:

1. Remove the driver's door panel (see page 20-7).
2. Disconnect the 2P connector from the actuator.

3. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

Passenger's door:

1. Remove the passenger's door panel (see page 20-7).
2. Disconnect the 2P connector from the actuator.

FRONT:

REAR:

3. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.