## Doors

#### Rear Door Weatherstrip Replacement

20-23

Rear Door Upper Seal Replacement

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. At the centre pillar, remove the door stop mounting bolt (A).

   Fastener Locations
   A : Bolt, 1 | B : Clip, 14

2. Detach the clip (B), then remove the door weatherstrip (C).
3. Install the weatherstrip in the reverse order of removal, and note these items:

- Replace any damaged clips.
- Make sure the weatherstrip is installed in the holder (D) securely.
- Apply liquid thread lock to the door stop mounting bolt before installation.
- Check for water leaks (see step 7 on page 20-25).

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. Remove the door sash trim (see page 20-22).
2. Detach the door weatherstrip clip (A), then remove the door upper seal (B).

   Fastener Location
   A : Clip, 1

3. Install the seal in the reverse order of removal, and note these items:

- Replace the clip if it's damaged.
- Make sure the upper seal is installed in the holder (C) securely.
- Check for water leaks (see step 7 on page 20-25).