## Steering

#### Steering Column Inspection

17-11

Except KX Model:

- Check the steering column ball bearing (A) and the steering joint bearing (B) for play and proper movement. If any bearing is noisy or has is excessive play, replace the steering column as an assembly.
- Check the sliding capsules (C) for distortion and breakage. If there is distortion or breakage replace the steering column as an assembly.

KX Model:

- Check the steering column ball bearing (A) and the steering joint bearing (B) for play and proper movement. If any bearing is noisy or has excessive play, replace the steering column as an assembly.
- Check the absorbing plate's (C), absorbing plate guides (D), stop (E) and coating plate's (F) for distortion or breakage. If there is distortion or breakage replace the steering column as an assembly.