## Driveline/Axle

#### Driveshaft Reassembly

16-2

Exploded View

1. INBOARD JOINT
2. CIRCLIP
3. (Right driveshaft)
4. ROLLER
5. DOUBLE LOOP BAND

   Replace.

   (Replacement parts only)

6. INBOARD BOOT

   Pack cavity with grease.

7. EAR CLAMP BAND

   Replace.

8. LOW PROFILE BAND

   Replace.

9. EAR CLAMP BAND

   Replace.

10. DRIVESHAFT
11. STOP RING

    Replace.

12. EAR CLAMPS BANDS

    Replace.

13. OUTBOARD JOINT
14. Pack cavity with grease.
15. OUTBOARD BOOT
16. Right driveshaft
17. DYNAMIC DAMPER

    (Undirectional)

18. Left driveshaft
19. SPIDER
20. Pack cavity with grease.
21. SET RING

    Replace.