## Seats

#### Front Seat Removal/Installation

20-229

For some models: SRS components are located in this area. Review the SRS component locations (see page 23-24) and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service. NOTE

- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to scratch the body or tear the seat covers.
- Put on gloves to protect your hands.

1. With side airbag, disconnect the negative battery cable and wait at least three minutes before beginning work.
2. Remove the seat track and covers (A) from the front of both seat tracks (B).

Outer:

Inner:

3. Remove the seat track end cover (A) from the back of both seat tracks.

Outer:

Inner: