## Plastic Parts Paint

#### Features of Plastic Material (cont'd)

6-12

Standard Symbol | Name | Heat Resistance Temperature °C (°F) | Solvent Resistance | Note
PP | Polypropylene | 80 (176) | Alcohol and gasoline are acceptable. | Solvent is not recommended.
PPO (PPE) | Polyphenylene oxide | 100 (212) | A small amount of alcohol is acceptable for a short time. | Soaking with an organic solvent such as gasoline and alcohol is not recommended.
PS | Polystyrene | 60 (140) | A small amount of alcohol is acceptable for a short time. | Soaking with an organic solvent such as gasoline and alcohol is not recommended.
PUR | Polyurethane | 80 (176) | A small amount of alcohol is acceptable for a short time. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol is not recommended.
PVC | Polyvinylchloride | 80 (176) | A small amount of alcohol and gasoline are acceptable for a short time. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol is not recommended.
SAN | Styrene acrylonitrile | 80 (176) | Wiping alcohol off in a short time can be allowed. | Soaking with an organic solvent such as gasoline and alcohol is not recommended.
SMC | Sheet moulding compound | 180 (356) | Alcohol and gasoline are acceptable. | Solvent is not recommended.
TPE | Thermoplastic polyester elastomer | 80 (176) | Alcohol is acceptable and wiping gasoline for a short time can be allowed. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol is not recommended. Wash remover off with water thoroughly.
TPS | Thermoplastic styrene elastomer | 80 (176) | A small amount of alcohol and gasoline are acceptable for a short time. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol is not recommended. Wash remover off with water thoroughly.
TPO | Thermoplastic olefin / elastomer | 80 (176) | Alcohol is acceptable and wiping gasoline for a short time can be allowed. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol is not recommended. Wash remover off with water thoroughly.
TPU | Thermoplastic / urethane / elastomer | 80 (176) | A small amount of alcohol and gasoline are acceptable for a short time. (Degreasing) | Soaking with an organic solvent such as gasoline and alcohol is not recommended. Wash remover off with water thoroughly.
UP | Polyester | 110 (230) | Alcohol and gasoline are acceptable. | Alkali is not recommended.