## Doors

#### Front Door Outer Handle Replacement

20-147

6. On driver's and some passenger's: Release the retainer clip (A), then remove the lock cylinder (B). Disconnect the cylinder rod (C).

7. With cylinder switch: Remove the screw, then separate the lock cylinder (A) and cylinder switch (B).

   Fastener Location
   : Screw, 1

8. With cylinder switch: Disconnect the cylinder switch connector (A) and detach the harness clips (B), then remove the cylinder switch (C).

9. If equipped with a outer handle protector, disconnect the outer handle rod (A).

   Fastener Locations
   : Bolt, 2

10. Remove the maintenance cap (B), and remove the bolts securing the outer handle (C). If equipped, release the hook (D), then remove the outer handle protector (E).