## Console

#### Centre Console Removal/Installation

20-73

NOTE:

- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to scratch the front seat, dashboard, and related parts.

1. Detach the clips (A, B) by pulling the centre console box (C) up, and if equipped, disconnect the seat heater switch connector (D), from the centre console (E).

   Fastener Locations
   A : Clip, 4 | B: Clip, 5

2. M/T: Remove the shift knob.

3. Remove the screws (A, B) and clips (C), and remove the centre console (D).

   Fastener Locations
   A : Screw, 2 | B : Screw, 2 | C : Clip, 2

4. Install the console in the reverse order of removal, and replace any damaged clips.