## Frame

#### Frame Repair Chart (cont'd)

20-273

l | Locating hole Ø25 (0.98) | T | For upper arm bracket centre Ø15 (0.98)
m | For trailing arm Ø13 (0.51) | U1, u2 | Locating hole Ø13 (0.51)
n | Locating hole Ø25 (0.98) | V | For upper arm Ø13 (0.51)
o | Locating hole Ø20 (0.79) | W | Locating hole Ø25 (0.98)
p | Trailing arm centre | X | For rear lower arm centre
q | Rear damper centre 73 x 68 (Slot) | Y | Locating hole Ø50 (1.97)
r | For upper arm Ø13 (0.51) | Z | Locating hole Ø20 (0.79)
s | For trailing arm Ø23 (0.51) |  |