## Driveline/Axle

#### Driveshafts Disassembly

16-5

Special Tools Required

- Threaded adapter, 22 x 1.5 mm 07XAC-0010100
- Slide hammer 07936-5790001
- Boot band pincers, commercially available

Inboard Joint Side:

1. Remove the set ring (A) from the inboard joint.

1. Remove the boot bands. Be careful not to damage the boot.

- If the boot band is a double loop type (A), lift up the band band (B) and push it into the clip (C).
- If the boot band is a low profile type (D), lift up the two tabs (E) with a screwdriver and pinch the boot band using the commercially available boot band pincer (F).
- It the boot band is an ear clamp type (G), lift up the three tabs (H) with a screwdriver.

Double Loop Type

Low Profile Type

Ear Clamp Type

a a a