## Manual Transmission

#### Gearshift Mechanism Replacement

13-48

4-door model:

1. SHIFT LEVER KNOB

   8 Nm (0.8 kgf/m, 5.8 lbf/ft)

2. SHIFT LEVER HOUSING
3. COTTER PIN

   Replace.

4. WASHER
5. SELECT LOCK PIN
6. COTTER PIN

   Replace.

7. Rotate the shift cable toward the opening.
8. SHIFT CABLE
9. Remove the shift cable from the shift lever bracket.
10. SHIFT CABLE CAP

    Replace.

11. SHIFT CABLE CLIP

    Replace.

12. COTTER PINS

    Replace.