## Exterior Lights

#### Taillight Replacement

22-118

Taillights (4-door):

1. Remove the rear bumper (see page 20-105).
2. Remove the trunk side trim panel (see page 20-67).
3. Open the trunk lid and disconnect the connectors (A) from the taillight (B).

   Brake/Taillight: | 21/5 W
   Turn Signal Light: | 21 W

4. Turn the bulb socket 45º counter-clockwise to remove the bulb socket.
5. Remove the mounting nuts and bolts, then remove the taillight.
6. When installing the taillight, check for the gasket; if it is distorted or stays compressed, replace it.
7. After installing the taillight, run water over the taillight to make sure they do not leak.

Inner Taillights (4-door):

1. Open the trunk lid and disconnect the connectors (A) from the inner taillight (B).

   Back-up Light: | 21 W
   Inner Taillight: | 5 W

2. Turn the bulb socket 45º counter-clockwise to remove the bulb socket.
3. Remove the mounting nuts, then remove the taillight.
4. When installing the taillight, check for the gasket; if it is distorted or stays compressed, replace it.
5. After installing the taillight, run water over the taillight to make sure they do not leak.