## Manual Transmission

#### Transmission Installation (cont'd)

13-11

1. Support subframe with a 4 X 4 X 40 in. piece of wood and a jack.

1. Install the front suspension subframe (A) in its original position by aligning the marks (B) you made in the removal procedure.

1. Loosely tighten the front engine mount bracket mounting bolt.

1. Install the three mounting bolts for the transmission rear mount.

a a a