## Interior Trim

#### Headliner Removal/Installation (cont'd)

20-70

Carpet Replacement

6. If necessary, remove the bolts, then remove the grab handle bracket (A). Remove the remaining grab handle brackets, as needed.

   Fastener Locations
   : Bolt, 6

7. Install the headliner in the reverse order of removal, and note these items:

- When reinstalling the headliner through the door opening, be careful not to fold or bend it. Also, be careful not to scratch the body.
- If the threads on a visor and grab handle screws are worn out, use an oversized self-tapping ET screw made specifically for this application.
- Check that both sides of the headliner are securely attached to the trim.

SRS components are located in this area. Review the SRS component locations (see page 23-23), and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service.

NOTE:

- Put on gloves to protect your hands.
- Take care not to damage, wrinkle or twist the carpet.
- Be careful not to damage the dashboard or other interior trim pieces.

1. Remove these items:

- Front seats, both sides (see page 20-87)
- Rear seat cushion, folding type (see page 20-95), fixed type (see page 20-96)
- Rear seat side bolsters, both sides, folding type (see page 20-95)
- Kick panels, both sides (see page 20-64)
- Front door sill trim, both sides (see page 20-64)
- Seat side trim, both sides (see page 20-64)
- Centre console (see page 20-73)
- Driver's dashboard under cover (see page 20-76)
- Passenger's dashboard lower cover (see page 20-78)

2. LHD: Remove the nut (A), and using a hex wrench, release the clip (B), then remove the footrest (C).

   Fastener Locations
   A : Nut, 1 | B : Clip, 1