## Driveline/Axle

#### Driveshafts Reassembly

16-2

Exploaded View

D16V1 engine model:

1. SET RING

   Replace.

2. INBOARD JOINT
3. CIRCLIP
4. ROLLER
5. SPIDER
6. INBOARD BOOT

   Pack cavity with grease.

7. DOUBLE LOOP BAND

   Replace.

8. Pack cavity with grease.
9. Left driveshaft
10. LOW PROFILE BAND

    Replace.

11. DRIVESHAFT
12. STOP RING

    Replace.

13. EAR CLAMP BANDS

    Replace.

14. OUTBOARD JOINT
15. Pack cavity with grease.
16. OUTBOARD BOOT (TPE)
17. Right driveshaft
18. DYNAMIC DAMPER

    (Undirectional)

a a a