## Engine Assembly

#### Engine Installation (cont'd)

5-11

2. Position the engine under the vehicle. Attach the chain hoist to the engine, then lift the engine into position in the vehicle.

Reinstall the mounting bolts/support nuts in the sequence given. Failure to follow this sequence may cause excessive noise and vibration and reduce bushing life.

3. Install the sub-frame (A). Align the reference lines (B) on the sub-frame with the bolt head centre, then tighten the bolts.

4. Tighten the rear mount mounting bolts.

5. Lower the hoist.
6. Tighten the side engine mount bracket mounting nuts.