## Glass

#### Windshield Replacement (cont'd)

20-20

12. Glue the side rubber dams (A), lower rubber dam (B) and fasteners (C) to the inside face of the windshield (D) as shown:

- Be sure the rubber dam and fasteners and dashboard seal line up with the alignment marks (E).
- Be careful not to touch the windshield where adhesive will be applied.

13. Glue the moulding (A) with adhesive tape (B) to the upper edge of the windshield (C):

- Be sure the alignment mark (D) of the moulding lines up with the alignment mark (E) of the windshield.
- Be careful not to touch the windshield where adhesive will be applied.

14. After installing the moulding, glue the seal (F) on each side of the moulding. Be sure the seal lines up with the edge of the rubber dam (G).
15. Install the clips (A) and retainers (B) to the body.

    Fastener Locations

    A : Clip, 2B : Retainer, 10