## Exterior Trim

#### Roof Moulding Replacement

20-115

1. Apply protective tape to the body (A). Using a flat-tip screwdriver wrapped with protective tape (B), pry up on the roof moulding (C). Take care not to scratch the body.

2. Pull up and slide the roof moulding to release the front bracket (D) from the pin (E).
3. Pull up the front portion of roof moulding.

4. Pull up and release the rear bracket (A) from the pin (B), then remove the roof moulding (C).

5. Install the moulding in the reverse order of removal, and note these items:

- Take care not to damage the windshield moulding.
- Make sure the roof moulding is installed securely.