## Cylinder Head

#### Camshaft Inspection (cont'd)

6-17

9. Check the total runout with the camshaft supported on V-blocks.

- If the total runout of the camshaft is within the service limit, replace the cylinder head.
- If the total runout is beyond the service limit, replace the camshaft and recheck the camshaft-to-holder oil clearance. If the oil clearance is still out of tolerance, replace the cylinder head.

Camshaft Total Runout:

Standard (New):0.03 mm (0.001 in.) max.

Service Limit:0.04 mm (0.002 in.)

10. Measure cam lobe height.

    Cam Lobe Height Standard (New):

    | INTAKE | EXHAUST
    D14Z6 engine | 34.158 mm (1.3448 in.) | 36.488 mm (1.4365 in.)
    D16V1, D16V3 engines | PRI | 38.427 mm (1.5129 in.) | 38.784 mm (1.5269 in.)
    SEC | 32.848 mm (1.2932 in.)

PRI: PrimarySEC: Secondary

IN: IntakeEX: ExhaustT/B: Timing Belt

D16V1, D16V3 engines: