## Security System

#### Door Key Cylinder Switch Test

22-264

4-door:

1. Remove the door panel (see page 20-7).
2. Disconnect the 3P connector from the key cylinder switch.

Wire side of female terminals

3. Check for continuity between the terminals.

- There should be continuity between the No. 2 and No. 3 terminals when the door key cylinder switch is LOCK position.
- There should be continuity between the No. 1 and No. 2 terminals when the door key cylinder switch is UNLOCK position.

5-door:

1. Remove the door panel (see page 20-144).
2. Disconnect the 3P connector from the key cylinder switch.

Wire side of female terminals

3. Check for continuity between the terminals.

- There should be continuity between the No. 2 and No. 3 terminals when the door key cylinder switch is LOCK position.
- There should be continuity between the No. 1 and No. 2 terminals when the door key cylinder switch is UNLOCK position.