## Keyless/Power Door Lock System

#### Door Lock Actuator Test (cont'd)

22-237
Tailgate Lock Actuator Test

5-door with Super Locking:

1. Remove the driver's door panel (see page 20-209).
2. Disconnect the 6 P connector from the actuator.

3. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

1. Remove the tailgate trim panel (see page 20-209).

2. Open the tailgate.
3. Disconnect the 2P[4P]connector from the tailgate lock actuator.

   [ ]: With super locking

4. Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.