## Cylinder Head

#### Cylinder Head Installation (cont'd)

6-21

17. Loosely install the alternator.
18. Adjust the alternator belt tension, refer to the '01 Civic Shop Manual on this CD (see page 4-38) or the alternator-compressor belt tension, refer to the '01 Civic Shop Manual on this CD (see page 4-37).
19. Install the connecting pipe (A) with new O-ring (B).

20. Install the water bypass hose (C).

21. Install the ground cable (A), upper radiator hose (B), lower radiator hose (C), heater hose (D) and water bypass hose (E).

22. Install the EVAP canister hose.