## Intake Manifold and Exhaust System

#### Exhaust Pipe and Muffler Replacement (cont'd)

9-4

NOTE: Use new gaskets and self-locking nuts when reassembling.

D17A5 engine:

1. GASKET, Replace.
2. MUFFLER
3. 8 x 1.25 mm, 22 Nm (2.2 kgf/m, 16 lbf/ft), Replace.

   Tighten the bolts in steps, alternating side-to-side.

4. HEAT SHIELD
5. EXHAUST PIPE B
6. GASKET, Replace.
7. EXHAUST PIPE A
8. 8 x 1.25 mm, 22 Nm (2.2 kgf/m, 16 lbf/ft), Replace.

   Tighten the bolts in steps, alternating side-to-side.

9. GASKET, Replace.
10. SELF-LOCKING NUT

    10 x 1.25 mm, 33 Nm (3.4 kgf/m, 25 lbf/ft), Replace.